switch / Timers

Mechanical day time switch with reserve power, 1 NO, 230 V AC

Electro-mechanical time switch with high accuracy rate and reserve.
Time programmes: daily program
 Time switch functions: Manual operation possible, potential-free switching contact
Switching interval: min. 15 min ... max. 24 h
Time range control gear: 24
Power reserve: 150 h

load circuit (relays):
1 NO
Rated voltage (AC): 250 V
Rated current AC (typ.): 16 A 
Rated frequency: 50 Hz ... 60 Hz 

Operating voltage (AC): 230 V

Operating position: optional

Housing type: distribution board housing
Installation type: Mounting rail (35 mm)
Protection class: IP20
Dimensions of transformer opening: W 18 mm (1 MW (module width)) × H 90 mm × D 66 mm

Design requirements/Standards: EN 60529, EN 60335-1

Factory: Doepke or similar
Item designation: Uno QRD
Order number: 09800034
selected make/type: ___________/___________