protect / Miniature circuit-breaker (MCB)

MCBs, C-characteristic, 25 A/230 V AC, 6 kA

Miniature circuit-breakers (MCB) in compact design for export
space saving installation, switching position indicator red/green, protection against wires being lodged behind terminals, extensive range of accessories retrofittable
 
Tripping characteristic: C
Number of poles: 1+N

load circuit (load disconnect contact):
Number of poles (total): 2
Rated voltage (AC): 230 V
Rated current AC (typ.): 25 A 
Rated frequency: 50 Hz, 60 Hz
Rated switching capacity as of EN 60898 at 230 V: 6 kA

screw-type terminal top and bottom (load circuit):
Cross section solid: 1-wire: 1 mm² ... 10 mm²
Cross section stranded: 1-wire: 1 mm² ... 10 mm²

 Ambient temperature: min. -25 °C ... max. 50 °C

Housing type: distribution board housing
Installation type: Mounting rail (35 mm)
Protection class: IP40
Dimensions of transformer opening: W 17.8 mm (1 MW (module width)) × H 80 mm × D 72 mm

Design requirements/Standards: EN 60898-1

Factory: Doepke or similar
Item designation: ELS 3 C25/1+N
Order number: 09915036
selected make/type: ___________/___________