expand / Operating current/undervoltage trips

Operating current trip for DLS 6

Shunt release for retrofitting the Doepke DLS 6 series

Shunt release:
suitable for device class: Miniature circuit-breakers
suitable for model range: DLS 6
Mounting side: right
maximum number of poles of main contact unit: 4
maximum current of main contact unit: 63 A 

Housing type: distribution board housing
Installation type: Mounting rail (35 mm), Device extension
Protection class: IP20 (installed: IP40)
Dimensions of transformer opening: W 17.5 mm (1 MW (module width)) × H 83 mm × D 75.2 mm

Factory: Doepke or similar
Item designation: DASA 12
Order number: 09917992
selected make/type: ___________/___________