expand / Wiring components

Busbar, fork, 2-pole, 63 A, 10 mm², 1010 mm, can be cut to length

RCCB and MCB busbars can be cut to length 1000 mm, cut-to-length
Specification connection: fork
Module widths: 56
Phase arrangement: L1, L2
Rail cross-section: 10 mm²
Modular dimension, rail: 17.8
Length: 1010 mm
Rated voltage AC (fix): 500 V
Rated current AC (typ.): 63 A
Dielectric constant: 4

Factory: Doepke or similar
Item designation: GM.2.56.100/10
Order number: 09920301
selected make/type: ___________/___________