switch / Float switches

Float switches (empty), Connection cable 5 m, rubber cable, protective conductor

Float switches for fill level monitoring
Function: empty

load circuit (switching contact):
1 NO
Number of poles (total): 1
Rated voltage (AC): 250 V
Rated current AC (typ.): 10 A 
Rated voltage: 250 V
Rated current: 10 A 
Cable type: H07RN-F 3G1
Length of connection cable: 5 m

Housing type: closed
Protection class: IP68
Dimensions of transformer opening: W 105 mm × H 81 mm × D 42 mm

Factory: Doepke or similar
Item designation: Champ 1 GS-L 05 m
Order number: 09921004
selected make/type: ___________/___________