protect / Fuse-switch-disconnectors

D0 fuse-switch-disconnectors Tytan, one-pole+N, 2 A - 63 A, with fuse monitoring

Main-fuse-switch-disconnectors for D01 and D02 fuses as empty housing with monitoring unit for the fuse

load circuit (switching contact):
2 NO
Number of poles (total): 2
Rated voltage (AC): 400 V 
max. Rated current AC: 63 A
Rated voltage (DC): max. 110 V
max. Total rated switching capacity: 50 kA
Rated insulation voltage: 690 V 

Electrical endurance: min. 1500 switching cycles
Mechanical endurance: min. 10000 switching cycles
Operating position: optional

Housing type: distribution board housing
Installation type: Mounting rail (35 mm)
Protection class: IP20 (installed: IP40)
Dimensions of transformer opening: W 81 mm (4.5 MW (module width)) × H 86 mm × D 70 mm

Design requirements/Standards: EN 60947-3

Factory: Doepke or similar
Item designation: Tytan II D0-63-1+N/M
Order number: 09980091
selected make/type: ___________/___________