expand / automatic reclosing devices

Remote actuator, 1 MW (module width),  24 V DC, RCCB: In max. 125 A, Switch-on attempts: 0

Retro-fittable unit for remote control and monitoring of Doepke residual current circuit-breakers from series DFS 2 and DFS 4.
Signals the tripped or disconnected status of the residual current circuit-breaker via a semiconductor output.
The remote actuator is operated via the push-button integrated on the front of the luminescent panel.
status display of the remote actuator via the front of the luminescent panel
extremely compact design with a module width of just 1.
Number of automatic switch-on attempts: 0
max. Rated current main contact unit: 125 A

control input:
Rated voltage (DC): 24 V (21.6 V ... 26.4 V)

switching output (semiconductor): 
Rated voltage (DC): 24 V (21.6 V ... 26.4 V)
Rated current DC (typ.): 0.2 A
max. Rated power: 4.8 VA

screw-type terminal top (control input, switching output):
Clamping area: min. 0.3 mm² ... max. 1.5 mm²

Operating voltage (DC): 24 V (21.6 V ... 26.4 V)
max. Current consumption DC: 2 A

Rated operating mode: continuous operation
Duty cycle: continuous operation
Operating position: optional

Housing type: distribution board housing
Installation type: Mounting rail (35 mm), Device extension
Protection class: IP20
Dimensions of transformer opening: W 17.3 mm (1 MW (module width)) × H 85 mm × D 73 mm

Design requirements/Standards: EN 55014, EN 63024

Factory: Doepke or similar
Item designation: DFA 3 024DC-0
Order number: 09100141
selected make/type: ___________/___________