monitor / Residual current analysis systems

Transducer for DRCA-1 set, 70 mm Ø (inner)

The transducers of series DRCA 1 CT together with the DRCA 1 detection unit form a residual current analysis system. Other detection units cannot be operated with this type of transformer. The transformers have a wide detection frequency range.

Residual current detection characteristic: A
: 
Frequency range response residual current Type A: 0 Hz ... 100 kHz
Current transformer suitable for: DRCA 1

transformer, primary side:
Rated voltage (AC): 0 V ... 690 V
Rated current: 200 A
Rated frequency: 10 Hz ... 100 kHz
Rated impulse withstand voltage: 8 kV / Kategorie IV  

Housing type: wall-mounted housing
Installation type: Wall mounting
Protection class: IP20
Dimensions of transformer opening: W 120 mm × H 129 mm × D 71 mm
Inside diameter: 70 mm

Design requirements/Standards: EN 61010-1, VDE 0411 Part 1

Factory: Doepke or similar
Item designation: DRCA 1 CT 070
Order number: 09352058
selected make/type: ___________/___________