switch / Twilight switches

Twilight switches, 24 V AC/DC, 10 A, signal white

Twilight switch 1 lux - 200 lux for wall and mast mounting
Adjustability, switch-on threshold twilight: Smooth, logarithmic
Switch-on threshold range shading twilight: 1 lux ... 200 lux
Twilight switch-off threshold range shading: 1 lux ... 200 lux
Adjustability of the switch-off threshold hysteresis factor: 1.5
Switch-on delay range: max. 10 s
Switch-off delay range: max. 40 s

load circuit (relays):
1 NO
Number of poles: 1
Rated voltage (AC): 230 V
Rated current AC (typ.): 10 A 
Rated frequency: 50 Hz
max. Rated power: 2500 VA

Operating voltage (AC): 24 V (21.6 V ... 26.4 V)
Operating frequency (fixed): 50 Hz
Operating voltage (DC): 24 V (21.6 V ... 26.4 V)
Housing colour: signal white (ähnlich RAL 9003)

Housing type: wall-mounted housing
Installation type: Mast assembly
Protection class: IP54
Dimensions of transformer opening: W 70 mm × H 90 mm × D 53 mm

Certifications: VDE
Design requirements/Standards: EN 60669-1

Factory: Doepke or similar
Item designation: Dasy 010-2 24 V AC/DC - we
Order number: 09500041
selected make/type: ___________/___________