expand / Wiring components

Busbar, fork, 1-pole, 4 MW (module width), 63 A (L1 x 4)

RCCB and MCB busbars Eurovario-System nach EN 60664-1, 500 V, 10 mm², fork
Specification connection: fork
Module widths: 4
Phase arrangement: L1 x 4
Rail cross-section: 10 mm²
Modular dimension, rail: 17.8
Length: 76 mm
Rated voltage AC (fix): 500 V
Rated current AC (typ.): 63 A
Dielectric constant: 4

Factory: Doepke or similar
Item designation: EV-S G 1.4.70
Order number: 09920126
selected make/type: ___________/___________