expand / Wiring components

DAFDD busbar, fork, 2-pole, 10 mm²

DAFDD busbars for DAFDD arc fault detection devices
Specification connection: fork
Module widths: 12
Phase arrangement: (L, N, S) x 4
Rail cross-section: 10 mm²
Modular dimension, rail: 17.8
Length: 202 mm
Rated voltage AC (fix): 500 V
Rated current AC (typ.): 63 A
Neutral conductor existent

Factory: Doepke or similar
Item designation: B G12TE-1/N/S-10
Order number: 09920130
selected make/type: ___________/___________