expand / Wiring components

DAFDD busbar, fork, 4-pole, can be cut to length, 10 mm²

DAFDD busbars for DAFDD arc fault detection devices
Specification connection: fork
Module widths: 60
Phase arrangement: L1, N, S, L2, N, S, L3, N, S, L1, …
Rail cross-section: 10 mm²
Modular dimension, rail: 17.8
Length: 1016 mm
Rated voltage AC (fix): 500 V
Rated current AC (typ.): 63 A
Neutral conductor existent

Factory: Doepke or similar
Item designation: B G60TE-3/N/S-10
Order number: 09920133
selected make/type: ___________/___________