expand / Wiring components

Busbar, fork, 3-pole, 8.5 MW (module width), 63 A (L1-Hi, L2-Hi, L3-Hi) x 2)

RCCB and MCB busbars Eurovario-System nach EN 60664-1, 500 V, 10 mm², fork
Specification connection: fork
Module widths: 8.5
Phase arrangement: L1-Hi, L2-Hi, L3-Hi) x 2
Rail cross-section: 10 mm²
Modular dimension, rail: 17.8
Length: 157 mm
Rated voltage AC (fix): 500 V
Rated current AC (typ.): 63 A
Auxiliary switch usable
Dielectric constant: 4

Factory: Doepke or similar
Item designation: EV-S G 3.1+Hi.6.120
Order number: 09920178
selected make/type: ___________/___________