expand / Wiring components

Busbar, fork, 3-pole, 12 MW (module width), 63 A (L1, L2, L3-N + L2, L3 + (L1, L2, L3) x 2)

RCCB and MCB busbars Eurovario-System nach EN 60664-1, 500 V, 10 mm², fork
Specification connection: fork
Module widths: 12
Phase arrangement: L1, L2, L3-N + L2, L3 + (L1, L2, L3) x 2
Rail cross-section: 10 mm²
Modular dimension, rail: 17.8
Length: 210 mm
Rated voltage AC (fix): 500 V
Rated current AC (typ.): 63 A
Neutral conductor existent
Dielectric constant: 4

Factory: Doepke or similar
Item designation: EV-S G 3/N.8.120
Order number: 09920185
selected make/type: ___________/___________