expand / Wiring components

Busbar, fork, 4-pole, 63 A, 10 mm², 965 mm, can be cut to length

RCCB and MCB busbars can be cut to length 1000 mm, cut-to-length
Specification connection: fork
Module widths: 54
Phase arrangement: L1+N, L2+N, L3+N
Rail cross-section: 10 mm²
Modular dimension, rail: 17.8
Length: 965 mm
Rated voltage AC (fix): 500 V
Rated current AC (typ.): 63 A
Neutral conductor existent
Dielectric constant: 4

Factory: Doepke or similar
Item designation: GM.4.54.100/10/N
Order number: 09920310
selected make/type: ___________/___________