expand / Wiring components

Busbar, fork, 4-pole, 80 A, 16 mm², 1032 mm, can be cut to length

RCCB and MCB busbars can be cut to length 1000 mm, cut-to-length
Specification connection: fork
Module widths: 52
Phase arrangement: L1, L2, L3, N
Rail cross-section: 16 mm²
Modular dimension, rail: 17.8
Length: 1032 mm
Rated voltage AC (fix): 500 V
Rated current AC (typ.): 80 A
Neutral conductor existent
Dielectric constant: 4

Factory: Doepke or similar
Item designation: GM.4+Hi.52/16
Order number: 09920318
selected make/type: ___________/___________