switch / Float switches

Float switches (fill/empty), Connection cable 20 m, rubber cable

Float switches for fill level monitoring
Function: fill/empty

load circuit (switching contact):
1 CO
Number of poles (total): 1
Rated voltage (AC): 250 V
Rated current AC (typ.): 10 A 
Rated voltage: 250 V
Rated current: 10 A 
Cable type: H07RN-F 3X1
Length of connection cable: 20 m

Housing type: closed
Protection class: IP68
Dimensions of transformer opening: W 105 mm × H 81 mm × D 42 mm

Factory: Doepke or similar
Item designation: Champ 2 G-L/F 20 m
Order number: 09921019
selected make/type: ___________/___________