protect / residual current operated circuit-breakers with integral overcurrent protection (RCBOs)

Residual current operated circuit-breaker with integral overcurrent protection, three-pole+N, 40 A, 0.03 A, B-Characteristic, Type A

Mains voltage-independent residual current circuit-breaker with overcurrent protection (RCBO) for detection of AC residual currents and pulsating DC residual currents
suitable for retro-fitting of additional equipment

Tripping characteristic: B
Residual current type: A
Rated residual current I&Delta;n: 0.03 A
Neutral conductor position: right
Module widths: 5

load circuit (load disconnect contact):
Number of poles: 4
Rated voltage (AC): 230 V, 400 V
Rated current AC (typ.): 40 A 
Rated frequency: 50 Hz, 60 Hz
max. total rated switching capacity: 6 kA
Rated insulation voltage: 440 V

screw-type terminal top, bottom (load circuit):
Cross section solid: 1-wire: 1 mm² ... 35 mm²
Cross section stranded: 1-wire: 1 mm² ... 25 mm²; 2-wire: 1 mm² ... 10 mm²
Connecting capacity flexible: 1-wire: 1 mm² ... 25 mm²
 Ambient temperature: min. -25 °C ... max. 40 °C

Housing type: distribution board housing
Installation type: Mounting rail (35 mm)
Protection class: IP20 (installed: IP40)
Dimensions of transformer opening: W 90 mm (5 MW (module width)) × H 92 mm × D 74 mm

Design requirements/Standards: EN 61009-1, EN 61009-2-1, VDE 0664-20

Factory: Doepke or similar
Item designation: FIB 40/0,03/3+N-A
Order number: 09955108
selected make/type: ___________/___________