protect / Fuse-switch-disconnectors

D0 fuse-switch-disconnectors Tytan, three-pole, 63 A, With flashing indicator in fuse plug, without fuse

Main-fuse-switch-disconnectors for D01 and D02 fuses with coloured fitted cartridge and fuse plug according to the specified rated current.

load circuit (switching contact):
3 NO
Number of poles (total): 3
Rated voltage (AC): 400 V
Rated current AC (typ.): 63 A 
Rated voltage (DC): max. 220 V
Rated short-circuit current: 50 kA
Rated insulation voltage: 690 V 

Electrical endurance: min. 1500 switching cycles

Housing type: distribution board housing
Installation type: Mounting rail (35 mm)
Protection class: IP20C (behind front panel with inserted fuse plugs)
Dimensions of transformer opening: W 81 mm (4.5 MW (module width)) × H 86 mm × D 70 mm

Design requirements/Standards: EN 60947-3

Factory: Doepke or similar
Item designation: Tytan II D0-63-3/E
Order number: 09980100
selected make/type: ___________/___________