protect / Fuse-switch-disconnectors / series Tytan

D0 fuse-switch-disconnectors Tytan, one-pole, 6 A, With fuse plug, without fuse

Main-fuse-switch-disconnectors for D01 and D02 fuses with coloured fitted cartridge and fuse plug according to the specified rated current.

load circuit (switching contact):
1 NO
Number of poles: 1
Rated voltage (AC): 400 V
Rated current AC (typ.): 6 A 
Rated voltage (DC): max. 110 V
max. total rated switching capacity: 50 kA
Rated insulation voltage: 800 V 

Electrical endurance: min. 1500 switching cycles
Mechanical endurance: min. 10000 switching cycles
Operating position: optional

Housing type: distribution board housing
Installation type: Mounting rail (35 mm)
Protection class: IP20 (installed: IP40)
Dimensions of transformer opening: W 27 mm (1.5 MW (module width)) × H 86 mm × D 70 mm

Design requirements/Standards: EN 60947-3

Factory: Doepke or similar
Item designation: Tytan II D0-06-1/S
Order number: 09980387
selected make/type: ___________/___________