protect / Fuse-switch-disconnectors

D0 fuse-switch-disconnectors Coron, three-pole, 2 A - 63 A

Fuse-switch-disconnectors for D01 and D02 fuses
Fuse plugs with flashing indicator
suitable for D0 fuses (D01 with retaining spring)
finger and back-of-hand proof
Cross-section of 1.5 mm² to 35 mm²
lockable using conventional padlocks

load circuit (load disconnect contact):
3 NO
Number of poles (total): 3
Rated voltage (AC): 400 V 
max. Rated current AC: 63 A
Rated voltage (DC): max. 220 V
max. Rated current DC: 63 A
Rated short-circuit current: 50 kA
Rated insulation voltage: 690 V 

Operating voltage (AC): 60 V ... 400 V

Electrical endurance: min. 1500 switching cycles
Operating position: optional

Housing type: distribution board housing
Installation type: Mounting rail (35 mm)
Protection class: IP20C (behind front panel with inserted fuse plugs)
Dimensions of transformer opening: W 81 mm (4.5 MW (module width)) × H 86 mm × D 70 mm

Design requirements/Standards: EN 60947-3

Factory: Doepke or similar
Item designation: Coron 2 63-3
Order number: 09980673
selected make/type: ___________/___________