switch / Control switches

Control switches, 16 A, 1 NO, with LED

control switches

Operating voltage (AC): 230 V
Operating frequency (fixed): 50 Hz

control input:
Rated voltage (AC): 250 V

load circuit (switching contact):
1 NO
Number of poles (total): 1
Rated voltage (AC): 250 V
Rated current AC (typ.): 16 A 
Rated frequency: 50 Hz
max. Total rated switching capacity: 16 A
Rated short-circuit current: 0.02 kA

Housing type: distribution board housing
Installation type: Mounting rail (35 mm)
Protection class: IP40
Dimensions of transformer opening: W 18 mm (1 MW (module width)) × H 90 mm × D 65 mm

Design requirements/Standards: EN 60715, EN 60669-1, VDE 0632-1, EN 60068-1

Factory: Doepke or similar
Item designation: RSS 016-100L
Order number: 09981075
selected make/type: ___________/___________