expand / Wiring components

Busbar for DRCBO 4 type B/B+, fork, 2-pole, 10 mm², 12 MW (module width), 63 A

DRCBO 4-busbars For RCCB/MCB combinations DRCBO 4 type B and B+
Specification connection: fork
Module widths: 12
Phase arrangement: 5 x (L, N)
Rail cross-section: 10 mm²
Modular dimension, rail: 17.8
Length: 210 mm
Rated voltage AC (fix): 480 V
Rated current AC (typ.): 63 A
Neutral conductor existent

Factory: Doepke or similar
Item designation: BG2.5.10
Order number: 09920151
selected make/type: ___________/___________