expand / Wiring components

D0 busbar, pin, 3-pole, can be cut to length, 3 x 35 mm²

D0 busbar can be cut to length for D0 switch-disconnectors Tytan and Coron
Specification connection: pin
Module widths: 39
Phase arrangement: L1, L2, L3
Rail cross-section: 35 mm²
Modular dimension, rail: 27
Length: 1050 mm
Rated voltage AC (fix): 500 V
Rated current AC (typ.): 125 A
Neutral conductor existent

Factory: Doepke or similar
Item designation: B S039-3-35/125 D0
Order number: 09980097
selected make/type: ___________/___________