expand / Wiring components

D0 busbar, pin, 1-pole, can be cut to length, 1 x 16 mm²

D0 busbar can be cut to length for D0 switch-disconnectors Tytan and Coron
Specification connection: pin
Module widths: 37
Phase arrangement: L1
Rail cross-section: 16 mm²
Modular dimension, rail: 27
Length: 990 mm
Rated voltage AC (fix): 500 V
Rated current AC (typ.): 80 A

Factory: Doepke or similar
Item designation: B S037-1-16/080 D0
Order number: 09980141
selected make/type: ___________/___________