expand

Fuse plug set, 40 A, green, mechanical, 230 V, 400 V AC

►The fuse plug sets of this series are suitable for Tytan II fuse-switch-disconnectors. Your box can be easily installed on the mounting rail and thus be used as a reserve box.▼Fuse plug sets of this series are accessories to Tytan II fuse-switch-disconnectors and consist of three plugs, three fitting cartridges and three fuses of the respective variant. The box has a rear bracket for snapping on a mounting rail, which enables it to be used as spare box in a distribution board.◄
This series of fuse plug sets contains fuses with mechanical display.

load circuit:
Number of poles (total): 1
Rated current AC (typ.): 40 A 

Housing type: distribution board housing
Installation type: Mounting rail (35 mm)
Dimensions of transformer opening: W 54 mm × H 45 mm × D 74 mm 
Housing colour: green

Design requirements/Standards: EN 60715, EN 50022, VDE 0110, VDE 0638, EN 60947

Factory: Doepke or similar
Item designation: DSE D02-40 MI
Order number: 09980641
selected make/type: ___________/___________